<?xml version="1.0" encoding="UTF-8"?>
<wave_config>
   <wave_state>
   </wave_state>
   <db_ref_list>
      <db_ref path="/home/aaron/Dokumente/STUDIUM/SEM6/EloSys/EloSysDigital/Projekt/vhdl-yasg/lcd_driver_tb_isim_beh.wdb" id="1" type="auto">
         <top_modules>
            <top_module name="lcd_driver_tb" />
            <top_module name="numeric_std" />
            <top_module name="std_logic_1164" />
         </top_modules>
      </db_ref>
   </db_ref_list>
   <WVObjectSize size="17" />
   <wvobject fp_name="/lcd_driver_tb/clk" type="logic" db_ref_id="1">
      <obj_property name="ElementShortName">clk</obj_property>
      <obj_property name="ObjectShortName">clk</obj_property>
   </wvobject>
   <wvobject fp_name="/lcd_driver_tb/reset" type="logic" db_ref_id="1">
      <obj_property name="ElementShortName">reset</obj_property>
      <obj_property name="ObjectShortName">reset</obj_property>
   </wvobject>
   <wvobject fp_name="/lcd_driver_tb/uut/busy" type="logic" db_ref_id="1">
      <obj_property name="ElementShortName">busy</obj_property>
      <obj_property name="ObjectShortName">busy</obj_property>
   </wvobject>
   <wvobject fp_name="/lcd_driver_tb/lcd_db" type="array" db_ref_id="1">
      <obj_property name="ElementShortName">lcd_db[7:0]</obj_property>
      <obj_property name="ObjectShortName">lcd_db[7:0]</obj_property>
   </wvobject>
   <wvobject fp_name="/lcd_driver_tb/data" type="array" db_ref_id="1">
      <obj_property name="ElementShortName">data[7:0]</obj_property>
      <obj_property name="ObjectShortName">data[7:0]</obj_property>
   </wvobject>
   <wvobject fp_name="/lcd_driver_tb/new_character" type="logic" db_ref_id="1">
      <obj_property name="ElementShortName">new_character</obj_property>
      <obj_property name="ObjectShortName">new_character</obj_property>
   </wvobject>
   <wvobject fp_name="/lcd_driver_tb/new_pos" type="logic" db_ref_id="1">
      <obj_property name="ElementShortName">new_pos</obj_property>
      <obj_property name="ObjectShortName">new_pos</obj_property>
   </wvobject>
   <wvobject fp_name="/lcd_driver_tb/uut/lcd_en" type="logic" db_ref_id="1">
      <obj_property name="ElementShortName">lcd_en</obj_property>
      <obj_property name="ObjectShortName">lcd_en</obj_property>
   </wvobject>
   <wvobject fp_name="/lcd_driver_tb/uut/lcd_rs" type="logic" db_ref_id="1">
      <obj_property name="ElementShortName">lcd_rs</obj_property>
      <obj_property name="ObjectShortName">lcd_rs</obj_property>
   </wvobject>
   <wvobject fp_name="/lcd_driver_tb/clk_period" type="other" db_ref_id="1">
      <obj_property name="ElementShortName">clk_period</obj_property>
      <obj_property name="ObjectShortName">clk_period</obj_property>
   </wvobject>
   <wvobject fp_name="/lcd_driver_tb/uut/cur_state" type="other" db_ref_id="1">
      <obj_property name="ElementShortName">cur_state</obj_property>
      <obj_property name="ObjectShortName">cur_state</obj_property>
   </wvobject>
   <wvobject fp_name="/lcd_driver_tb/uut/next_state" type="other" db_ref_id="1">
      <obj_property name="ElementShortName">next_state</obj_property>
      <obj_property name="ObjectShortName">next_state</obj_property>
   </wvobject>
   <wvobject fp_name="/lcd_driver_tb/uut/ret_state" type="other" db_ref_id="1">
      <obj_property name="ElementShortName">ret_state</obj_property>
      <obj_property name="ObjectShortName">ret_state</obj_property>
   </wvobject>
   <wvobject fp_name="/lcd_driver_tb/uut/next_ret_state" type="other" db_ref_id="1">
      <obj_property name="ElementShortName">next_ret_state</obj_property>
      <obj_property name="ObjectShortName">next_ret_state</obj_property>
   </wvobject>
   <wvobject fp_name="/lcd_driver_tb/uut/cur_counter" type="array" db_ref_id="1">
      <obj_property name="ElementShortName">cur_counter[20:0]</obj_property>
      <obj_property name="ObjectShortName">cur_counter[20:0]</obj_property>
      <obj_property name="Radix">UNSIGNEDDECRADIX</obj_property>
   </wvobject>
   <wvobject fp_name="/lcd_driver_tb/uut/ret_counter" type="array" db_ref_id="1">
      <obj_property name="ElementShortName">ret_counter[20:0]</obj_property>
      <obj_property name="ObjectShortName">ret_counter[20:0]</obj_property>
      <obj_property name="Radix">UNSIGNEDDECRADIX</obj_property>
   </wvobject>
   <wvobject fp_name="/lcd_driver_tb/uut/cur_lcd_db" type="array" db_ref_id="1">
      <obj_property name="ElementShortName">cur_lcd_db[7:0]</obj_property>
      <obj_property name="ObjectShortName">cur_lcd_db[7:0]</obj_property>
   </wvobject>
</wave_config>
